2024/5/27 16:29:32 新建项目11成功
2024/5/27 16:29:33 通讯(COM1)连接成功
2024/5/27 16:30:24 Current project(11)Loading…
2024/5/27 16:30:25 Current project(11)download finished
2024/5/27 16:30:25 Communication(COM1)Connection succeeded
7/7/2025 4:49:38 PM New project 123 succeeded
7/7/2025 4:49:38 PM Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
7/7/2025 4:49:54 PM Communication connection failed, unable to read the function code of the current page
7/7/2025 4:49:56 PM Communication connection failed, unable to read the function code of the current page
07/14/2025 14:43:37 New project 11 succeeded
07/14/2025 14:43:38 Communication(COM9)Connection succeeded
07/14/2025 14:43:41 Communication(COM9)Disconnected
07/14/2025 14:43:44 Successfully modify the communication parameter configuration
07/14/2025 14:44:00 Communication(COM8)Abnormal connection：Please check the parameters of the serial port configurationПревышен таймаут семафора.

07/14/2025 15:13:55 Successfully modify the communication parameter configuration
07/14/2025 15:13:56 Communication(COM9)Connection succeeded
07/14/2025 15:14:13 Communication(COM9)Disconnected
07/14/2025 15:14:19 Successfully modify the communication parameter configuration
07/14/2025 15:14:20 Communication(COM7)Connection succeeded
07/14/2025 15:15:45 Read function code(C00.00 Given frequency)：0.00
07/14/2025 15:15:45 Read function code(C00.01 Output frequency)：0.00
07/14/2025 15:15:45 Read function code(C00.02 Output current)：0.0
07/14/2025 15:15:45 Read function code(C00.03 Input voltage)：344.2
07/14/2025 15:15:45 Read function code(C00.04 Output voltage)：0.0
07/14/2025 15:15:45 Read function code(C00.05 Mechanical speed)：0
07/14/2025 15:15:45 Read function code(C00.06 Given torque)：250.0
07/14/2025 15:15:45 Read function code(C00.07 Output torque)：0.0
07/14/2025 15:15:45 Read function code(C00.08 PID Given amount)：0.0
07/14/2025 15:15:45 Read function code(C00.09 PID Feedback amount)：0.0
07/14/2025 15:15:45 Read function code(C00.10 Output Power)：0.0
07/14/2025 15:15:45 Read function code(C00.11 Bus voltage)：487.6
07/14/2025 15:15:45 Read function code(C00.12 Module temperature1)：30.9
07/14/2025 15:15:45 Read function code(C00.13 Module temperature2)：30.9
07/14/2025 15:15:46 Read function code(C00.14 Input terminal X connected state)：00000000
07/14/2025 15:15:46 Read function code(C00.15 Output terminal Y connected state)：00000000
07/14/2025 15:15:46 Read function code(C00.16 Analog AS input value)：0.000
07/14/2025 15:15:46 Read function code(C00.17 Analog VS input value)：0.000
07/14/2025 15:15:46 Read function code(C00.18 Keyboard potentiometer)：0.00
07/14/2025 15:15:46 Read function code(C00.19 Pulse signal PUL input value)：0.000
07/14/2025 15:15:46 Read function code(C00.20 Analog output AO1)：0.00
07/14/2025 15:15:46 Read function code(C00.21 Analog output AO2 (extended))：0.00
07/14/2025 15:15:46 Read function code(C00.22 Counter count value)：0
07/14/2025 15:15:46 Read function code(C00.23 Running time of this power-on)：0.0
07/14/2025 15:15:46 Read function code(C00.24 Accumulated running time of this machine)：0
07/14/2025 15:15:46 Read function code(C00.25 Inverter power rated power)：0.7
07/14/2025 15:15:46 Read function code(C00.26 Inverter rated voltage)：380
07/14/2025 15:15:46 Read function code(C00.27 Inverter rated current)：3.0
07/14/2025 15:15:46 Read function code(C00.28 Software version)：23.06
07/14/2025 15:15:46 Read function code(C00.29 PGFeedback frequency)：0.00
07/14/2025 15:15:46 Read function code(C00.30 Timer )：513
07/14/2025 15:15:46 Read function code(C00.31 PID output )：0.00
07/14/2025 15:15:46 Read function code(C00.32 Software subversion)：0.01
07/14/2025 15:15:46 Read function code(C00.33 Encoder angle)：231.30
07/14/2025 15:15:46 Read function code(C00.34 Z pulse error)：513
07/14/2025 15:15:46 Read function code(C00.35 Z pulse count)：0
07/14/2025 15:15:46 Read function code(C00.36 Fault warning code)：0:No failure
07/14/2025 15:15:46 Read function code(C00.37 Cumulative power consumption (low level))：0
07/14/2025 15:15:46 Read function code(C00.38 Accumulated electricity consumption (high　level))：0
07/14/2025 15:15:46 Read function code(C00.39 Power factor angle)：0.0
07/14/2025 15:15:46 Read function code(C00.40)：0
07/14/2025 15:15:47 Read function code(C00.41)：0
07/14/2025 15:15:47 Read function code(C00.42)：0
07/14/2025 15:15:47 Read function code(C00.43)：0
07/14/2025 15:15:47 Read function code(C00.44)：0
07/14/2025 15:15:47 Read function code(C00.45)：0
07/14/2025 15:15:47 Read function code(C00.46)：0
07/14/2025 15:15:47 Read function code(C00.47)：0
07/14/2025 15:15:47 Read function code(C00.48)：0
07/14/2025 15:15:47 Read function code(C00.49)：0
07/14/2025 15:15:47 Read function code(C00.50)：0
07/14/2025 15:15:47 Read function code(C00.51)：0
07/14/2025 15:15:47 Read function code(C00.52)：0
07/14/2025 15:15:47 Read function code(C00.53)：0
07/14/2025 15:15:47 Read function code(C00.54)：25000
07/14/2025 15:15:47 Read function code(C00.55)：0
07/14/2025 15:15:48 Read function code(C00.56)：0
07/14/2025 15:15:48 Read function code(C00.57)：65524
07/14/2025 15:15:48 Read function code(C00.58)：65524
07/14/2025 15:15:48 Read function code(C00.59)：0
07/14/2025 15:15:48 Read function code(C00.60)：4870
07/14/2025 15:15:48 Read function code(C00.61)：0
07/14/2025 15:15:48 Read function code(C00.62)：0
07/14/2025 15:15:48 Read function code(C00.63)：0
07/14/2025 15:15:53 Read function code(C02.00 PID given )：0.0
07/14/2025 15:15:53 Read function code(C02.01 PID feedback )：0.0
07/14/2025 15:15:53 Read function code(C02.02 PID output )：0.00
07/14/2025 15:15:53 Read function code(C02.03 PID status )：0
07/14/2025 15:15:53 Read function code(C02.04 Reserved)：896.0
07/14/2025 15:15:53 Read function code(C02.05 PLC number of current running segments )：0
07/14/2025 15:15:53 Read function code(C02.06 PLC current Output frequency)：0.00
07/14/2025 15:15:53 Read function code(C02.07 Reserved)：0.0
07/14/2025 15:15:53 Read function code(C02.08 Forward and reverse command given )：0
07/14/2025 15:15:53 Read function code(C02.09 Jog command given )：0
07/14/2025 15:15:54 Read function code(C02.10 AS adjusted by curve )：0.000
07/14/2025 15:15:54 Read function code(C02.11 VS adjusted by curve )：0.000
07/14/2025 15:15:54 Read function code(C02.12 Reserved)：0.000
07/14/2025 15:15:54 Read function code(C02.13 Reserved)：0.000
07/14/2025 15:15:54 Read function code(C02.14 Reserved)：00000000
07/14/2025 15:15:54 Read function code(C02.15 Inverter overload timing)：0.0
07/14/2025 15:15:54 Read function code(C02.16 Motor overload timing)：0.0
07/14/2025 15:15:54 Read function code(C02.17 Reserved)：0.00
07/14/2025 15:15:54 Read function code(C02.18 Reserved)：2.0
07/14/2025 15:15:54 Read function code(C02.19 Accumulated number of wave-by-wave current limiting)：0
07/14/2025 15:15:54 Read function code(C02.20 Serial port received frame number )：1.04
07/14/2025 15:15:54 Read function code(C02.21 CRC check error count )：0.00
07/14/2025 15:15:54 Read function code(C02.22 Serial port error count )：22
07/14/2025 15:15:54 Read function code(C02.23 Number of current frames received )：0.0
07/14/2025 15:15:54 Read function code(C02.24 Number of current frames sent)：65535
07/14/2025 15:15:54 Read function code(C02.25 Inverter status 1)：0.0
07/14/2025 15:15:54 Read function code(C02.26 Inverter status 2)：0
07/14/2025 15:15:54 Read function code(C02.27 Inverter status 3)：0.0
07/14/2025 15:15:54 Read function code(C02.28 Extension terminal status )：00000000
07/14/2025 15:15:54 Read function code(C02.29 Motor temperature )：0.0
07/14/2025 15:15:54 Read function code(C02.30 Reserved)：0
07/14/2025 15:15:55 Read function code(C02.31 Reserved)：0
07/14/2025 15:15:55 Read function code(C02.32 Power-down storage parameter 1)：0
07/14/2025 15:15:55 Read function code(C02.33 Power-down storage parameter 2)：0
07/14/2025 15:15:55 Read function code(C02.34 Power-down storage parameter 3)：0
07/14/2025 15:15:55 Read function code(C02.35 Power-down storage parameter 4)：0
07/14/2025 15:15:55 Read function code(C02.36 Power-down storage parameter 5)：0
07/14/2025 15:15:55 Read function code(C02.37 Power-down storage parameter 6)：0
07/14/2025 15:15:55 Read function code(C02.38 Power-down storage parameter 7)：0
07/14/2025 15:15:55 Read function code(C02.39 Power-down storage parameter 8)：0
07/14/2025 15:15:55 Read function code(C02.40 Power-down storage parameter 9)：0
07/14/2025 15:15:55 Read function code(C02.41 Power-down storage parameter 10)：0
07/14/2025 15:15:55 Read function code(C02.42 Power-down storage parameter 11)：0
07/14/2025 15:15:55 Read function code(C02.43 Power-down storage parameter 12)：0
07/14/2025 15:15:55 Read function code(C02.44 Power-down storage parameter 13)：0
07/14/2025 15:15:55 Read function code(C02.45 Power-down storage parameter 14)：0
07/14/2025 15:15:55 Read function code(C02.46 Power-down storage parameter 15)：0
07/14/2025 15:15:55 Read function code(C02.47 Power-down storage parameter 16)：0
07/14/2025 15:15:55 Read function code(C02.48 Reserved)：0
07/14/2025 15:15:55 Read function code(C02.49 Reserved)：0
07/14/2025 15:15:55 Read function code(C02.50 Cache Register 0)：0
07/14/2025 15:15:55 Read function code(C02.51 Cache Register 1)：0
07/14/2025 15:15:55 Read function code(C02.52 Cache Register 2)：0
07/14/2025 15:15:55 Read function code(C02.53 Cache Register 3)：0
07/14/2025 15:15:55 Read function code(C02.54 Cache Register 4)：0
07/14/2025 15:15:55 Read function code(C02.55 Cache Register 5)：0
07/14/2025 15:15:55 Read function code(C02.56 Cache Register 6)：0
07/14/2025 15:15:56 Read function code(C02.57 Cache Register 7)：0
07/14/2025 15:15:56 Read function code(C02.58 Cache Register 8)：0
07/14/2025 15:15:56 Read function code(C02.59 Cache Register 9)：0
07/14/2025 15:15:56 Read function code(C02.60 Expansion port A Software version)：601
07/14/2025 15:15:56 Read function code(C02.61 Expansion port B Software version)：128
07/14/2025 15:15:56 Read function code(C02.62 External keyboard Software version)：0
07/14/2025 15:15:56 Read function code(C02.63 Reserved )：0
07/14/2025 15:16:03 Read function code(F00.00 Parameter access level )：0:Standard parameter 
07/14/2025 15:16:03 Read function code(F00.01 Purpose selection)：0:Universal 
07/14/2025 15:16:03 Read function code(F00.02 Reserved )：0
07/14/2025 15:16:03 Read function code(F00.03 Initialization)：0:Not initialized 
07/14/2025 15:16:03 Read function code(F00.04 Keyboard parameter copy)：0:No function 
07/14/2025 15:16:03 Read function code(F00.05 User password)：0000
07/14/2025 15:16:03 Read function code(F00.06 Reserved)：0
07/14/2025 15:16:03 Read function code(F00.07 Free parameter 1)：0
07/14/2025 15:16:03 Read function code(F00.08 Free parameter 2)：0
07/14/2025 15:16:03 Read function code(F00.09 Reserved)：0
07/14/2025 15:16:03 Read function code(F00.10 Common parameters 1Address setting)：0100
07/14/2025 15:16:03 Read function code(F00.11 Common parameters 2Address setting)：0101
07/14/2025 15:16:03 Read function code(F00.12 Common parameters 3Address setting)：0102
07/14/2025 15:16:03 Read function code(F00.13 Common parameters 4Address setting)：0710
07/14/2025 15:16:03 Read function code(F00.14 Common parameters 5Address setting)：0122
07/14/2025 15:16:03 Read function code(F00.15 Common parameters 6Address setting)：0123
07/14/2025 15:16:03 Read function code(F00.16 Common parameters 7Address setting)：0110
07/14/2025 15:16:04 Read function code(F00.17 Common parameters 8Address setting)：0112
07/14/2025 15:16:04 Read function code(F00.18 Common parameters 9Address setting)：0140
07/14/2025 15:16:04 Read function code(F00.19 Common parameters 10Address setting)：0730
07/14/2025 15:16:04 Read function code(F00.20 Common parameters 11Address setting)：0201
07/14/2025 15:16:04 Read function code(F00.21 Common parameters 12Address setting)：0202
07/14/2025 15:16:04 Read function code(F00.22 Common parameters 13Address setting)：0203
07/14/2025 15:16:04 Read function code(F00.23 Common parameters 14Address setting)：0204
07/14/2025 15:16:04 Read function code(F00.24 Common parameters 15Address setting)：0205
07/14/2025 15:16:04 Read function code(F00.25 Common parameters 16Address setting)：0206
07/14/2025 15:16:04 Read function code(F00.26 Common parameters 17Address setting)：0207
07/14/2025 15:16:04 Read function code(F00.27 Common parameters 18Address setting)：1201
07/14/2025 15:16:04 Read function code(F00.28 Common parameters 19Address setting)：1202
07/14/2025 15:16:04 Read function code(F00.29 Common parameters 20Address setting)：1203
07/14/2025 15:16:04 Read function code(F00.30 Common parameters 21Address setting)：0700
07/14/2025 15:16:04 Read function code(F00.31 Common parameters 22Address setting)：0705
07/14/2025 15:16:04 Read function code(F00.32 Common parameters 23Address setting)：0502
07/14/2025 15:16:04 Read function code(F00.33 Common parameters 24Address setting)：0503
07/14/2025 15:16:05 Read function code(F00.34 Common parameters 25Address setting)：0504
07/14/2025 15:16:05 Read function code(F00.35 Common parameters 26Address setting)：0601
07/14/2025 15:16:05 Read function code(F00.36 Common parameters 27Address setting)：0600
07/14/2025 15:16:05 Read function code(F00.37 Common parameters 28Address setting)：0621
07/14/2025 15:16:05 Read function code(F00.38 Common parameters 29Address setting)：0622
07/14/2025 15:16:05 Read function code(F00.39 Common parameters 30Address setting)：0400
07/14/2025 15:16:05 Read function code(F00.40 Single board debugging options)：0000
07/14/2025 15:16:05 Read function code(F00.41 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.42 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.43 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.44 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.45 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.46 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.47 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.48 Reserved)：0
07/14/2025 15:16:05 Read function code(F00.49 Reserved)：0
07/14/2025 15:16:07 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
07/14/2025 15:16:07 Read function code(F01.01 Run command channel)：2:RS485 communication control
07/14/2025 15:16:07 Read function code(F01.02 Frequency setting source channel A)：6:RS485 communication given
07/14/2025 15:16:07 Read function code(F01.03 Frequency setting source channel A gain)：100.0
07/14/2025 15:16:07 Read function code(F01.04 Frequency source channel B gain)：3:Voltage analog VS given
07/14/2025 15:16:07 Read function code(F01.05Frequency feed source channel B gain)：100.0
07/14/2025 15:16:07 Read function code(F01.06 Frequency channel B reference source)：0:Maximum output frequency as reference source
07/14/2025 15:16:07 Read function code(F01.07 Frequency feed source selection)：0:Channel A
07/14/2025 15:16:07 Read function code(F01.08 Run command bundle to set frequency)：0000
07/14/2025 15:16:07 Read function code(F01.09 Keypad numeric setting frequency)：33.00
07/14/2025 15:16:07 Read function code(F01.10 Maximum frequency)：50.00
07/14/2025 15:16:08 Read function code(F01.11 Upper limit frequency source selection)：0:Upper limit frequency digitally set
07/14/2025 15:16:08 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
07/14/2025 15:16:08 Read function code(F01.13 Lower limit frequency )：0.00
07/14/2025 15:16:08 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
07/14/2025 15:16:08 Read function code(F01.15 Reserved)：1
07/14/2025 15:16:08 Read function code(F01.16 Reserved)：50000
07/14/2025 15:16:08 Read function code(F01.17 Reserved)：4
07/14/2025 15:16:08 Read function code(F01.18 Reserved)：0
07/14/2025 15:16:08 Read function code(F01.19 Reserved)：0
07/14/2025 15:16:08 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
07/14/2025 15:16:08 Read function code(F01.21 Acceleration time unit)：2:0.01S
07/14/2025 15:16:08 Read function code(F01.22 Acceleration time 1)：5.00
07/14/2025 15:16:08 Read function code(F01.23 Deceleration time 1)：5.00
07/14/2025 15:16:08 Read function code(F01.24 Acceleration time 2)：10.00
07/14/2025 15:16:08 Read function code(F01.25 Deceleration time 2)：10.00
07/14/2025 15:16:08 Read function code(F01.26 Acceleration time 3)：10.00
07/14/2025 15:16:09 Read function code(F01.27 Deceleration time 3)：10.00
07/14/2025 15:16:09 Read function code(F01.28 Acceleration time 4)：10.00
07/14/2025 15:16:09 Read function code(F01.29 Deceleration time 4)：10.00
07/14/2025 15:16:09 Read function code(F01.30 S-curve acceleration/deceleration selection)：1:Valid
07/14/2025 15:16:09 Read function code(F01.31 Acceleration start S-curve time )：0.20
07/14/2025 15:16:09 Read function code(F01.32 Acceleration end S curve time )：0.20
07/14/2025 15:16:09 Read function code(F01.33 S-curve time to start deceleration )：0.20
07/14/2025 15:16:09 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
07/14/2025 15:16:09 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
07/14/2025 15:16:09 Read function code(F01.36 Reserved)：0
07/14/2025 15:16:09 Read function code(F01.37 Reserved)：0
07/14/2025 15:16:09 Read function code(F01.38 Reserved)：0
07/14/2025 15:16:09 Read function code(F01.39 Reserved)：0
07/14/2025 15:16:09 Read function code(F01.40 PWM Carrier frequency )：4.0
07/14/2025 15:16:09 Read function code(F01.41 PWM Control mode )：1111
07/14/2025 15:16:09 Read function code(F01.42 PWM way to control 1)：9101
07/14/2025 15:16:09 Read function code(F01.43 Dead zone compensation gain )：306
07/14/2025 15:16:09 Read function code(F01.44 Bootstrap time)：15
07/14/2025 15:16:09 Read function code(F01.45 Bootstrap protection time)：50
07/14/2025 15:16:09 Read function code(F01.46 Random carrier depth)：0
07/14/2025 15:16:09 Read function code(F01.47 Reserved)：0
07/14/2025 15:16:09 Read function code(F01.48 Reserved)：0.00
07/14/2025 15:16:10 Read function code(F01.49 Reserved)：6.0
07/14/2025 15:16:23 Set function code(F01.01 Run command channel)：2-->1:Terminal control
07/14/2025 15:16:39 Set function code(F00.03 Initialization)：0-->22:All Parameter initialization
07/14/2025 15:16:55 Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
07/14/2025 15:16:56 Read function code(F01.01 Run command channel)：1:Terminal control
07/14/2025 15:16:56 Read function code(F01.02 Frequency setting source channel A)：3:Voltage analog VS given
07/14/2025 15:16:56 Read function code(F01.03 Frequency setting source channel A gain)：100.0
07/14/2025 15:16:56 Read function code(F01.04 Frequency source channel B gain)：3:Voltage analog VS given
07/14/2025 15:16:56 Read function code(F01.05Frequency feed source channel B gain)：100.0
07/14/2025 15:16:56 Read function code(F01.06 Frequency channel B reference source)：0:Maximum output frequency as reference source
07/14/2025 15:16:56 Read function code(F01.07 Frequency feed source selection)：0:Channel A
07/14/2025 15:16:56 Read function code(F01.08 Run command bundle to set frequency)：0000
07/14/2025 15:16:56 Read function code(F01.09 Keypad numeric setting frequency)：50.00
07/14/2025 15:16:56 Read function code(F01.10 Maximum frequency)：50.00
07/14/2025 15:16:56 Read function code(F01.11 Upper limit frequency source selection)：0:Upper limit frequency digitally set
07/14/2025 15:16:56 Read function code(F01.12 Digital setting of upper limit frequency)：50.00
07/14/2025 15:16:56 Read function code(F01.13 Lower limit frequency )：0.00
07/14/2025 15:16:56 Read function code(F01.14 Frequency Instruction Resolution)：0:0.01Hz
07/14/2025 15:16:56 Read function code(F01.15 Reserved)：1
07/14/2025 15:16:56 Read function code(F01.16 Reserved)：50000
07/14/2025 15:16:56 Read function code(F01.17 Reserved)：4
07/14/2025 15:16:56 Read function code(F01.18 Reserved)：0
07/14/2025 15:16:56 Read function code(F01.19 Reserved)：0
07/14/2025 15:16:56 Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
07/14/2025 15:16:56 Read function code(F01.21 Acceleration time unit)：2:0.01S
07/14/2025 15:16:56 Read function code(F01.22 Acceleration time 1)：3.00
07/14/2025 15:16:56 Read function code(F01.23 Deceleration time 1)：3.00
07/14/2025 15:16:56 Read function code(F01.24 Acceleration time 2)：10.00
07/14/2025 15:16:56 Read function code(F01.25 Deceleration time 2)：10.00
07/14/2025 15:16:56 Read function code(F01.26 Acceleration time 3)：10.00
07/14/2025 15:16:56 Read function code(F01.27 Deceleration time 3)：10.00
07/14/2025 15:16:56 Read function code(F01.28 Acceleration time 4)：10.00
07/14/2025 15:16:56 Read function code(F01.29 Deceleration time 4)：10.00
07/14/2025 15:16:57 Read function code(F01.30 S-curve acceleration/deceleration selection)：1:Valid
07/14/2025 15:16:57 Read function code(F01.31 Acceleration start S-curve time )：0.20
07/14/2025 15:16:57 Read function code(F01.32 Acceleration end S curve time )：0.20
07/14/2025 15:16:57 Read function code(F01.33 S-curve time to start deceleration )：0.20
07/14/2025 15:16:57 Read function code(F01.34 S-curve time at the end of deceleration)：0.20
07/14/2025 15:16:57 Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
07/14/2025 15:16:57 Read function code(F01.36 Reserved)：0
07/14/2025 15:16:57 Read function code(F01.37 Reserved)：0
07/14/2025 15:16:57 Read function code(F01.38 Reserved)：0
07/14/2025 15:16:57 Read function code(F01.39 Reserved)：0
07/14/2025 15:16:57 Read function code(F01.40 PWM Carrier frequency )：4.0
07/14/2025 15:16:57 Read function code(F01.41 PWM Control mode )：1111
07/14/2025 15:16:57 Read function code(F01.42 PWM way to control 1)：9101
07/14/2025 15:16:57 Read function code(F01.43 Dead zone compensation gain )：306
07/14/2025 15:16:57 Read function code(F01.44 Bootstrap time)：15
07/14/2025 15:16:57 Read function code(F01.45 Bootstrap protection time)：50
07/14/2025 15:16:57 Read function code(F01.46 Random carrier depth)：0
07/14/2025 15:16:57 Read function code(F01.47 Reserved)：0
07/14/2025 15:16:57 Read function code(F01.48 Reserved)：0.00
07/14/2025 15:16:57 Read function code(F01.49 Reserved)：6.0
07/14/2025 15:16:59 Communication(COM7)Disconnected
07/14/2025 15:17:21 New project llkl succeeded
07/14/2025 15:17:22 Communication(COM9)Connection succeeded
07/14/2025 15:17:25 Communication(COM9)Disconnected
07/14/2025 15:17:29 Successfully modify the communication parameter configuration
07/14/2025 15:17:29 Communication(COM7)Connection succeeded
07/14/2025 15:18:00 The serial port is unplugged, please check the line
07/14/2025 15:18:00 Communication(COM7)Disconnected
07/15/2025 09:28:16 Current project(123)Loading…
07/15/2025 09:28:16 Current project(123)download finished
07/15/2025 09:28:16 Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
07/15/2025 09:28:26 New project 101 succeeded
07/15/2025 09:28:27 Communication(COM9)Connection succeeded
